|  |  |
| --- | --- |
| 3GPP TS 38.101-1 V16.12.1 (2022-06) | |
| Technical Specification | |
| 3rd Generation Partnership Project;  Technical Specification Group Radio Access Network;  NR;  User Equipment (UE) radio transmission and reception;  Part 1: Range 1 Standalone  (Release 16) | |
|  | |
| *5G-logo_175px* | 3GPP-logo_web |
|  | |
| The present document has been developed within the 3rd Generation Partnership Project (3GPP TM) and may be further elaborated for the purposes of 3GPP. The present document has not been subject to any approval process by the 3GPPOrganizational Partners and shall not be implemented. This Specification is provided for future development work within 3GPPonly. The Organizational Partners accept no liability for any use of this Specification. Specifications and Reports for implementation of the 3GPP TM system should be obtained via the 3GPP Organizational Partners' Publications Offices. | |

|  |
| --- |
|  |
| ***3GPP***  Postal address  3GPP support office address  650 Route des Lucioles - Sophia Antipolis  Valbonne - FRANCE  Tel.: +33 4 92 94 42 00 Fax: +33 4 93 65 47 16  Internet  http://www.3gpp.org |
| ***Copyright Notification***  No part may be reproduced except as authorized by written permission. The copyright and the foregoing restriction extend to reproduction in all media.  © 2022, 3GPP Organizational Partners (ARIB, ATIS, CCSA, ETSI, TSDSI, TTA, TTC).  All rights reserved.  UMTS™ is a Trade Mark of ETSI registered for the benefit of its members  3GPP™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners LTE™ is a Trade Mark of ETSI registered for the benefit of its Members and of the 3GPP Organizational Partners  GSM® and the GSM logo are registered and owned by the GSM Association |

Contents

Foreword 16

1 Scope 18

2 References 18

3 Definitions, symbols and abbreviations 18

3.1 Definitions 18

3.2 Symbols 19

3.3 Abbreviations 21

4 General 23

4.1 Relationship between minimum requirements and test requirements 23

4.2 Applicability of minimum requirements 23

4.3 Specification suffix information 23

5 Operating bands and channel arrangement 24

5.1 General 24

5.2 Operating bands 24

5.2A Operating bands for CA 26

5.2A.0 General 26

5.2A.1 Intra-band CA 26

5.2A.2 Inter-band CA 27

5.2A.2.1 Inter-band CA (two bands) 27

5.2A.2.2 Inter-band CA (three bands) 31

5.2A.2.3 Inter-band CA (four bands) 32

5.2B Operating bands for DC 32

5.2C Operating band combination for SUL 32

5.2D Operating bands for UL MIMO 33

5.2E Operating band for V2X 33

5.2E.1 V2X operating bands 33

5.2E.2 V2X operating bands for con-current operation 34

5.3 UE channel bandwidth 34

5.3.1 General 34

5.3.2 Maximum transmission bandwidth configuration 35

5.3.3 Minimum guardband and transmission bandwidth configuration 35

5.3.4 RB alignment 37

5.3.5 UE channel bandwidth per operating band 37

5.3.6 Asymmetric channel bandwidths 40

5.3A UE channel bandwidth for CA 41

5.3A.1 General 41

5.3A.2 Maximum transmission bandwidth configuration for CA 41

5.3A.3 Minimum guardband and transmission bandwidth configuration for CA 41

5.3A.4 Void 43

5.3A.5 UE channel bandwidth per operating band for CA 43

5.3E Channel bandwidth for V2X 44

5.3E.1 General 44

5.3E.2 Channel bandwidth for V2X concurrent operation 45

5.4 Channel arrangement 45

5.4.1 Channel spacing 45

5.4.1.1 Channel spacing for adjacent NR carriers 45

5.4.2 Channel raster 45

5.4.2.1 NR-ARFCN and channel raster 45

5.4.2.2 Channel raster to resource element mapping 46

5.4.2.3 Channel raster entries for each operating band 46

5.4.3 Synchronization raster 49

5.4.3.1 Synchronization raster and numbering 49

5.4.3.3 Synchronization raster entries for each operating band 50

5.4.4 TX–RX frequency separation 53

5.4A Channel arrangement for CA 53

5.4A.1 Channel spacing for CA 53

5.4A.2 Channel raster for CA 54

5.4A.3 Synchronization raster for CA 54

5.4A.4 Tx-Rx frequency separation for CA 54

5.4B Reserved 54

5.4C Reserved 54

5.4D Reserved 54

5.4E Channel arrangement for V2X 54

5.4E.1 Channel spacing 54

5.4E.2 Channel raster 55

5.4E.2.1 NR-ARFCN and channel raster 55

5.4E.2.2 Channel raster to resource element mapping 55

5.4E.2.3 Channel raster entries for each operating band 55

5.4E.3 Synchronization raster for V2X 55

5.5 Void 55

5.5A Configurations for CA 55

5.5A.0 General 55

5.5A.1 Configurations for intra-band contiguous CA 57

5.5A.2 Configurations for intra-band non-contiguous CA 60

5.5A.3 Configurations for inter-band CA 60

5.5A.3.1 Configurations for inter-band CA (two bands) 60

5.5A.3.2 Configurations for inter-band CA (three bands) 72

5.5A.3.3 Configurations for inter-band CA (four bands) 80

5.5B Configurations for DC 83

5.5C Configurations for SUL 84

6 Transmitter characteristics 84

6.1 General 84

6.1A General 84

6.1F General 84

6.2 Transmitter power 84

6.2.1 UE maximum output power 84

6.2.2 UE maximum output power reduction 86

6.2.3 UE additional maximum output power reduction 89

6.2.3.1 General 89

6.2.3.2 A-MPR for NS\_04 94

6.2.3.3 A-MPR for NS\_10 95

6.2.3.4 A-MPR for NS\_05 and NS\_05U 95

6.2.3.5 A-MPR for NS\_40 98

6.2.3.6 A-MPR for NS\_43 and NS\_43U 98

6.2.3.7 A-MPR for NS\_03 and NS\_03U 99

6.2.3.8 A-MPR for NS\_37 100

6.2.3.9 A-MPR for NS\_38 101

6.2.3.10 A-MPR for NS\_39 101

6.2.3.11 A-MPR for NS\_41 101

6.2.3.12 A-MPR for NS\_42 102

6.2.3.13 A-MPR for NS\_18 102

6.2.3.14 A-MPR for NS\_21 103

6.2.3.15 A-MPR for NS\_24 103

6.2.3.16 A-MPR for NS\_27 104

6.2.3.17 A-MPR for NS\_46 105

6.2.3.18 A-MPR for NS\_47 106

6.2.3.19 A-MPR for NS\_50 107

6.2.3.20 A-MPR for NS\_44 107

6.2.3.21 A-MPR for NS\_12 108

6.2.3.22 A-MPR for NS\_13 108

6.2.3.23 A-MPR for NS\_14 109

6.2.3.24 A-MPR for NS\_15 110

6.2.3.25 A-MPR for NS\_45 110

6.2.3.26 A-MPR for NS\_48 111

6.2.3.27 A-MPR for NS\_49 111

6.2.3.28 A-MPR for NS\_51 112

6.2.4 Configured transmitted power 113

6.2A Transmitter power for CA 115

6.2A.1 UE maximum output power for CA 115

6.2A.1.1 UE maximum output power for Intra-band contiguous CA 115

6.2A.1.2 UE maximum output power for Intra-band non-contiguous CA 115

6.2A.1.3 UE maximum output power for Inter-band CA 116

6.2A.1.4 Void 119

6.2A.1.5 Void 119

6.2A.2 UE maximum output power reduction for CA 119

6.2A.2.1 UE maximum output power reduction for Intra-band contiguous CA 119

6.2A.2.2 UE maximum output power reduction for Intra-band non-contiguous CA 121

6.2A.2.2.0 General 121

6.2A.2.2.1 MPR to meet -30dBm/MHz 121

6.2A.2.2.2 MPR to meet -13dBm/MHz 122

6.2A.2.3 UE maximum output power reduction for Inter-band CA 122

6.2A.2.4 Void 122

6.2A.3 UE additional maximum output power reduction for CA 122

6.2A.3.1.1 UE additional maximum output power reduction for Intra-band contiguous CA 122

6.2A.3.1.1.1 A-MPR for CA\_NS\_04 123

6.2A.3.1.2 UE additional maximum output power reduction for Intra-band non-contiguous CA 129

6.2A.3.1.3 UE additional maximum output power reduction for Inter-band CA 131

6.2A.4 Configured output power for CA 133

6.2A.4.1 Configured transmitted power level 133

6.2A.4.1.1 Configured transmitted power for Intra-band contiguous CA 133

6.2A.4.1.2 Configured transmitted power for Intra-band non-contiguous CA 135

6.2A.4.1.3 Configured transmitted power for Inter-band CA 137

6.2A.4.1.4 Void 139

6.2A.4.2 ΔTIB,c for CA 139

6.2A.4.2.1 Void 139

6.2A.4.2.2 Void 139

6.2A.4.2.3 ΔTIB,c for Inter-band CA (two bands) 139

6.2A.4.2.4 ΔTIB,c for Inter-band CA (three bands) 144

6.2A.4.2.5 ΔTIB,c for Inter-band CA (four bands) 147

6.2B Transmitter power for NR-DC 147

6.2B.0 General 147

6.2B.1 UE maximum output power for NR-DC 147

6.2B.2 UE maximum output power reduction for NR-DC 148

6.2B.3 UE additional maximum output power reduction for NR-DC 148

6.2B.4 Configured output power for NR-DC 148

6.2B.4.1 Configured transmitted power level for NR-DC 148

6.2B.4.2 ΔTIB,c for NR-DC 151

6.2C Transmitter power for SUL 151

6.2C.1 Configured transmitted power for SUL 151

6.2C.2 ΔTIB,c 151

6.2D Transmitter power for UL MIMO 152

6.2D.1 UE maximum output power for UL MIMO 152

6.2D.2 UE maximum output power reduction for UL MIMO 153

6.2D.3 UE additional maximum output power reduction for UL MIMO 154

6.2D.4 Configured transmitted power for UL MIMO 154

6.2E Transmitter power for V2X 155

6.2E.1 UE maximum output power for V2X 155

6.2E.1.1 General 155

6.2E.1.2 UE maximum output power for V2X con-current operation 156

6.2E.2 UE maximum output power reduction for V2X 156

6.2E.2.1 General 156

6.2E.2.2 MPR for Power class 3 V2X UE 156

6.2E.2.3 MPR for Power class 3 V2X con-current operation 157

6.2E.3 UE additional maximum output power reduction for V2X 157

6.2E.3.1 General 157

6.2E.3.2 A-MPR for Power class 3 V2X UE by NS\_33 158

6.2E.3.3 A-MPR for Power class 3 V2X UE by NS\_52 160

6.2E.3.4 A-MPR for power class 3 V2X con-current operation 161

6.2E.4 Configured transmitted power for V2X 161

6.2E.4.1 General 161

6.2E.4.2 Configured transmitted power for V2X con-current operation 162

6.2F Transmitter power for shared spectrum channel access 163

6.2F.1 UE maximum output power 163

6.2F.1A UE maximum output power for CA 164

6.2F.1A.1 UE maximum output power for inter-band CA 164

6.2F.2 UE maximum output power reduction 164

6.2F.2A UE maximum output power reduction for CA 165

6.2F.2A.1 UE maximum output power reduction for inter-band CA 165

6.2F.3 UE additional maximum output power reduction 165

6.2F.3.1 General 165

6.2F.3.2 A-MPR for NS\_28 166

6.2F.3.3 A-MPR for NS\_29 167

6.2F.3.4 A-MPR for NS\_30 167

6.2F.3.5 A-MPR for NS\_31 168

6.2F.3.6 A-MPR for NS\_53 168

6.2F.3.7 A-MPR for NS\_54 169

6.2F.3A UE additional maximum output power reduction for CA 169

6.2F.3A.1 UE additional maximum output power reduction for inter-band CA 169

6.2F.4 Configured transmitted power 170

6.3 Output power dynamics 170

6.3.1 Minimum output power 170

6.3.2 Transmit OFF power 170

6.3.3 Transmit ON/OFF time mask 171

6.3.3.1 General 171

6.3.3.2 General ON/OFF time mask 171

6.3.3.3 Transmit power time mask for slot and short or long subslot boundaries 171

6.3.3.4 PRACH time mask 172

6.3.3.5 Void 173

6.3.3.6 SRS time mask 173

6.3.3.7 PUSCH-PUCCH and PUSCH-SRS time masks 174

6.3.3.8 Transmit power time mask for consecutive slot or long subslot transmission and short subslot transmission boundaries 176

6.3.3.9 Transmit power time mask for consecutive short subslot transmissions boundaries 176

6.3.4 Power control 177

6.3.4.1 General 177

6.3.4.2 Absolute power tolerance 177

6.3.4.3 Relative power tolerance 178

6.3.4.4 Aggregate power tolerance 178

6.3A Output power dynamics for CA 178

6.3A.1 Minimum output power for CA 178

6.3A.1.1 Minimum output power for intra-band contiguous CA 178

6.3A.1.2 Minimum output power for intra-band non-contiguous CA 179

6.3A.1.3 Minimum output power for inter-band CA 179

6.3A.1.4 Void 179

6.3A.2 Transmit OFF power for CA 179

6.3A.2.1 Transmit OFF power for intra-band contiguous CA 179

6.3A.2.2 Transmit OFF power for intra-band non-contiguous CA 179

6.3A.2.3 Transmit OFF power for inter-band CA 179

6.3A.2.4 Void 179

6.3A.3 Transmit ON/OFF time mask for CA 179

6.3A.3.1 Transmit ON/OFF time mask for intra-band contiguous CA 179

6.3A.3.2 Transmit ON/OFF time mask for intra-band non-contiguous CA 180

6.3A.3.3 Transmit ON/OFF time mask for inter-band CA 180

6.3A.3.3.1 General 180

6.3A.3.3.2 Time mask for switching between two uplink carriers 180

6.3A.3.4 Void 181

6.3A.4 Power control for CA 181

6.3A.4.1 Power control for intra-band contiguous CA 181

6.3A.4.1.1 Absolute power tolerance 181

6.3A.4.1.2 Relative power tolerance 181

6.3A.4.1.3 Aggregate power control tolerance 182

6.3A.4.2 Power control for intra-band non-contiguous CA 182

6.3A.4.2.1 Absolute power tolerance 182

6.3A.4.2.1.1 Minimum requirements 182

6.3A.4.2.2 Relative power tolerance 182

6.3A.4.2.2.1 Minimum requirements 182

6.3A.4.2.3 Aggregate power control tolerance 182

6.3A.4.3 Power control for inter-band CA 182

6.3A.4.4 Void 182

6.3B Output power dynamics for NR-DC 182

6.3C Output power dynamics for SUL 183

6.3C.1 Void 183

6.3C.2 Void 183

6.3C.3 Transmit ON/OFF time mask for SUL 183

6.3C.3.1 Time mask for switching between two uplink carriers 183

6.3D Output power dynamics for UL MIMO 184

6.3D.1 Minimum output power for UL MIMO 184

6.3D.2 Transmit OFF power for UL MIMO 184

6.3D.3 Transmit ON/OFF time mask for UL MIMO 184

6.3D.4 Power control for UL MIMO 184

6.3E Output power dynamics for V2X 184

6.3E.1 Minimum output power for V2X 184

6.3E.1.1 General 184

6.3E.1.2 Minimum output power for V2X con-current operation 185

6.3E.2 Transmit OFF power for V2X 185

6.3E.2.1 General 185

6.3E.2.2 Transmit OFF power for V2X con-current operation 185

6.3E.3 Transmit ON/OFF time mask for V2X 185

6.3E.3.1 General 185

6.3E.3.2 General time mask 186

6.3E.3.3 S-SSB time mask 186

6.3E.3.4 Transmit ON/OFF time mask for V2X con-current operation 187

6.3E.4 Power control for V2X 187

6.3E.4.1 General 187

6.3E.4.2 Absolute power tolerance 187

6.3E.4.3 Power control for V2X con-current operation 187

6.3F Output power dynamics for shared spectrum channel access 187

6.3F.1 Minimum output power 187

6.3F.2 Transmit OFF power 187

6.3F.3 Transmit ON/OFF time mask 187

6.3F.3.1 General 187

6.3F.3.2 General ON/OFF time mask 187

6.3F.3A General ON/OFF mask for CA 188

6.3F.3A.1 General ON/OFF mask for inter-band CA 188

6.3F.4 Power control 188

6.3F.4.1 General 188

6.3F.4.2 Absolute power tolerance 188

6.3F.4.3 Relative power tolerance 188

6.3F.4.4 Aggregate power tolerance 188

6.4 Transmit signal quality 189

6.4.1 Frequency error 189

6.4.2 Transmit modulation quality 189

6.4.2.1 Error Vector Magnitude 189

6.4.2.1a Error Vector Magnitude including symbols with transient period 190

6.4.2.2 Carrier leakage 191

6.4.2.3 In-band emissions 191

6.4.2.4 EVM equalizer spectrum flatness 192

6.4.2.4.1 Requirements for Pi/2 BPSK modulation 193

6.4A Transmit signal quality for CA 194

6.4A.1 Frequency error for CA 194

6.4A.1.1 Frequency error for intra-band contiguous CA 194

6.4A.1.2 Frequency error for intra-band non-contiguous CA 194

6.4A.1.3 Frequency error for inter-band CA 194

6.4A.1.4 Void 195

6.4A.2 Transmit modulation quality for CA 195

6.4A.2.1 Transmit modulation quality for intra-band contiguous CA 195

6.4A.2.1.0 General 195

6.4A.2.1.1 Error Vector Magnitude 195

6.4A.2.1.2 In-band emissions 195

6.4A.2.1.3 Carrier leakage 198

6.4A.2.2 Transmit modulation quality for intra-band non-contiguous CA 198

6.4A.2.2.0 General 198

6.4A.2.2.1 Error Vector Magnitude 198

6.4A.2.2.2 In-band emissions 199

6.4A.2.2.3 Carrier leakage 199

6.4A.2.3 Transmit modulation quality for inter-band CA 199

6.4A.2.4 Void 199

6.4B Transmit signal quality for NR-DC 199

6.4D Transmit signal quality for UL MIMO 199

6.4D.1 Frequency error for UL MIMO 199

6.4D.2 Transmit modulation quality for UL MIMO 199

6.4D.2.1 Error Vector Magnitude 200

6.4D.2.2 Carrier leakage 200

6.4D.2.3 In-band emissions 200

6.4D.2.4 EVM equalizer spectrum flatness for UL MIMO 200

6.4D.3 Time alignment error for UL MIMO 200

6.4D.4 Requirements for coherent UL MIMO 200

6.4E Transmit signal quality for V2X 201

6.4E.1 Frequency error for V2X 201

6.4E.1.1 General 201

6.4E.1.2 Frequency error for V2X con-current operation 201

6.4E.2 Transmit modulation quality for V2X 201

6.4E.2.1 General 201

6.4E.2.2 Error Vector Magnitude for V2X 202

6.4E.2.3 Carrier leakage for V2X 202

6.4E.2.4 In-band emissions for V2X 202

6.4E.2.5 EVM equalizer spectrum flatness for V2X 202

6.4E.2.6 Transmit modulation quality for V2X con-current operation 202

6.4F Transmit signal quality for shared spectrum channel access 202

6.4F.1 Frequency error 202

6.4F.2 Transmit modulation quality 202

6.4F.2.1 Error Vector Magnitude 203

6.4F.2.2 Carrier leakage 203

6.4F.2.3 In-band emissions 203

6.4F.2.4 EVM equalizer spectrum flatness 204

6.4F.2A Transmit modulation quality for CA 204

6.4F.2A.1 Transmit modulation quality for inter-band CA 204

6.5 Output RF spectrum emissions 204

6.5.1 Occupied bandwidth 204

6.5.2 Out of band emission 205

6.5.2.1 General 205

6.5.2.2 Spectrum emission mask 205

6.5.2.3 Additional spectrum emission mask 206

6.5.2.3.1 Requirements for network signalling value "NS\_35" 206

6.5.2.3.2 Requirements for network signalling value "NS\_04" 206

6.5.2.3.3 Requirements for network signalling values "NS\_03", “NS\_03U”, and "NS\_21" 207

6.5.2.3.4 Requirements for network signalling value "NS\_06" 207

6.5.2.3.5 Void 208

6.5.2.3.6 Void 208

6.5.2.3.7 Void 208

6.5.2.3.8 Requirements for network signalling value "NS\_27" 208

6.5.2.4 Adjacent channel leakage ratio 208

6.5.2.4.1 NR ACLR 209

6.5.2.4.2 UTRA ACLR 209

6.5.3 Spurious emissions 210

6.5.3.1 General spurious emissions 210

6.5.3.2 Spurious emissions for UE co-existence 210

6.5.3.3 Additional spurious emissions 218

6.5.3.3.1 Requirement for network signalling value "NS\_04" 218

6.5.3.3.2 Requirement for network signalling value "NS\_17" 219

6.5.3.3.3 Requirement for network signalling value "NS\_18" 219

6.5.3.3.4 Requirement for network signalling values "NS\_05" and “NS\_05U” 219

6.5.3.3.5 Requirement for network signalling values "NS\_43" and “NS\_43U” 219

6.5.3.3.6 Requirement for network signalling value "NS\_37" 220

6.5.3.3.7 Requirement for network signalling value "NS\_38" 220

6.5.3.3.8 Requirement for network signalling value "NS\_39" 220

6.5.3.3.9 Requirement for network signalling value "NS\_40" 220

6.5.3.3.10 Requirement for network signalling value "NS\_41" 221

6.5.3.3.11 Requirement for network signalling value "NS\_42" 221

6.5.3.3.12 Requirement for network signalling value "NS\_21" 221

6.5.3.3.13 Requirement for network signalling value "NS\_24" 221

6.5.3.3.14 Requirement for network signalling value "NS\_27" 222

6.5.3.3.15 Requirement for network signalling value "NS\_47" 222

6.5.3.3.16 Requirement for network signalling value "NS\_50" 222

6.5.3.3.17 Requirement for network signalling value "NS\_12" 223

6.5.3.3.18 Requirement for network signalling value "NS\_13" 223

6.5.3.3.19 Requirement for network signalling value "NS\_14" 223

6.5.3.3.20 Requirement for network signalling value "NS\_15" 223

6.5.3.3.21 Requirement for network signalling value "NS\_45" 224

6.5.3.3.22 Requirement for network signalling values "NS\_48" and "NS\_51" 224

6.5.3.3.23 Requirement for network signalling value "NS\_49" 224

6.5.3.3.24 Requirement for network signalling value "NS\_44" 225

6.5.3.3.25 Requirement for network signalling value "NS\_46" 225

6.5.4 Transmit intermodulation 225

6.5A Output RF spectrum emissions for CA 226

6.5A.1 Occupied bandwidth for CA 226

6.5A.1.1 Void 226

6.5A.1.1a Occupied bandwidth for Intra-band contiguous CA 226

6.5A.1.2 Occupied bandwidth for Intra-band non-contiguous CA 226

6.5A.1.3 Occupied bandwidth for Inter-band CA 226

6.5A.2 Out of band emission for CA 226

6.5A.2.1 General 226

6.5A.2.2 Spectrum emission mask 227

6.5A.2.2.1 Spectrum emission mask for intra-band contiguous CA 227

6.5A.2.2.2 Spectrum emission mask for intra-band non-contiguous CA 227

6.5A.2.2.3 Spectrum emission mask for Inter-band CA 227

6.5.A.2.2.4 Void 227

6.5A.2.3 Additional spectrum emission mask for CA 227

6.5A.2.3.1 Additional spectrum emission mask for intra-band contiguous CA 227

6.5A.2.3.1 Void 228

6.5A.2.3.2 Additional spectrum emission mask for Intra-band non-contiguous CA 228

6.5A.2.3.2.1 Minimum requirement (network signalling value “CA\_NC\_NS\_04”) 228

6.5A.2.3.3 Additional spectrum emission mask for Inter-band CA 228

6.5A.2.4 Adjacent channel leakage ratio 228

6.5A.2.4.1 NR ACLR 228

6.5A.2.4.2 UTRA ACLR 230

6.5A.3 Spurious emission for CA 230

6.5A.3.1 General spurious emissions 230

6.5A.3.2 Spurious emissions for UE co-existence 231

6.5A.3.2.1 Spurious emissions for UE co-existence for intra-band contiguous CA 231

6.5A.3.2.2 Spurious emissions for UE co-existence for intra-band non-contiguous CA 232

6.5A.3.2.3 Spurious emissions for UE co-existence for Inter-band CA 232

6.5A.3.2.4 Void 242

6.5A.3.2.5 Void 242

6.5A.3.2.6 Void 242

6.5A.3.3 Additional spurious emissions for CA 242

6.5A.3.3.1 Additional spurious emissions for intra-band contiguous CA 242

6.5A.3.3.2 Additional spurious emissions for intra-band non-contiguous CA 243

6.5A.4 Transmit intermodulation for CA 243

6.5A.4.2.1 Transmit intermodulation for intra-band contiguous CA 243

6.5A.4.2.2 Void 243

6.5B Output RF spectrum emissions for NR-DC 243

6.5D Output RF spectrum emissions for UL MIMO 243

6.5D.1 Occupied bandwidth for UL MIMO 243

6.5D.2 Out of band emission for UL MIMO 244

6.5D.3 Spurious emission for UL MIMO 244

6.5D.4 Transmit intermodulation for UL MIMO 244

6.5E Output RF spectrum emissions for V2X 244

6.5E.1 Occupied bandwidth for V2X 244

6.5E.1.1 General 244

6.5E.1.2 Occupied bandwidth for V2X con-current operation 245

6.5E.2 Out of band emission for V2X 245

6.5E.2.1 General 245

6.5E.2.2 Spectrum emission mask 245

6.5E.2.2.1 General 245

6.5E.2.2.2 Spectrum emission mask for V2X con-current operation 245

6.5E.2.3 Additional Spectrum emission mask 245

6.5E.2.3.1 Requirements for network signalling value "NS\_33" 245

6.5E.2.3.2 Requirements for network signalling value "NS\_52" 246

6.5E.2.4 Adjacent channel leakage ratio 246

6.5E.2.4.1 General 246

6.5E.2.4.2 ACLR for V2X con-current operation 247

6.5E.3 Spurious emissions for V2X 247

6.5E.3.1 General spurious emissions 247

6.5E.3.2 Spurious emissions for UE co-existence 247

6.5E.3.3 Spurious emissions for UE co-existence for V2X con-current operation 247

6.5E.3.4 Additional spurious emissions requirements for V2X 248

6.5E.3.4.1 General 248

6.5E.3.4.2 Requirements for network signalling value "NS\_33" 248

6.5E.3.4.3 Void 249

6.5E.4 Transmit intermodulation 249

6.5E.4.1 General 249

6.5E.4.2 Transmit intermodulation for V2X con-current operation 249

6.5F Output RF spectrum emissions 249

6.5F.1 Occupied bandwidth 249

6.5F.2 Out of band emission 249

6.5F.2.1 General 249

6.5F.2.2 Spectrum emission mask for operation with shared spectrum channel access 249

6.5F.2.2.1 Spectrum emission mask for non-transmitted channels 250

6.5F.2.3 Additional spectrum emission mask 250

6.5F.2.4 Adjacent channel leakage ratio 250

6.5F.2.4.1 Shared spectrum channel access ACLR 251

6.5F.2.4.2 Additional requirement for network signaled value "NS\_29" 251

6.5F.3 Spurious emissions 251

6.5F.3.1 General spurious emissions 251

6.5F.3.2 Spurious emissions for UE co-existence 251

6.5F.3.3 Additional spurious emissions 251

6.5F.3.3.1 Requirement for network signalling value "NS\_28" 252

6.5F.3.3.2 Requirement for network signalling value "NS\_29" 252

6.5F.3.3.3 Requirement for network signalling value "NS\_30" 253

6.5F.3.3.4 Requirement for network signalling value "NS\_31" 254

6.5F.3.3.5 Requirements for network signalling value "NS\_53" or "NS\_54" 255

6.5F.4 Transmit intermodulation 255

6.6 Void 255

6.6E Time alignment error 255

7 Receiver characteristics 256

7.1 General 256

7.1A General 256

7.1F General 257

7.2 Diversity characteristics 257

7.3 Reference sensitivity 257

7.3.1 General 257

7.3.2 Reference sensitivity power level 257

7.3.3 ΔRIB,c 265

7.3A Reference sensitivity for CA 266

7.3A.1 General 266

7.3A.2 Reference sensitivity power level for CA 266

7.3A.2.1 Reference sensitivity power level for Intra-band contiguous CA 266

7.3A.2.2 Reference sensitivity power level for Intra-band non-contiguous CA 266

7.3A.2.3 Reference sensitivity power level for Inter-band CA 267

7.3A.2.4 Void 267

7.3A.3 ΔRIB,c for CA 267

7.3A.3.1 General 267

7.3A.3.2 ΔRIB,c for Inter-band CA 267

7.3A.3.2.1 ΔRIB,c for two bands 269

7.3A.3.2.2 Void 272

7.3A.3.2.3 ΔRIB,c for three bands 272

7.3A.3.2.4 ΔRIB,c for four bands 275

7.3A.4 Reference sensitivity exceptions due to UL harmonic interference for CA 275

7.3A.5 Reference sensitivity exceptions due to intermodulation interference due to 2UL CA 280

7.3A.6 Reference sensitivity exceptions due to cross band isolation for CA 286

7.3B Reference sensitivity for NR-DC 287

7.3C Reference sensitivity for SUL 287

7.3C.1 General 287

7.3C.2 Reference sensitivity power level for SUL 287

7.3C.3 ΔRIB,c for SUL 290

7.3C.3.1 General 290

7.3C.3.2 SUL band combination 290

7.3C.3.2.1 ΔRIB,c for two bands 291

7.3D Reference sensitivity for UL MIMO 291

7.3E Reference sensitivity for V2X 291

7.3E.1 General 291

7.3E.2 Minimum requirements 291

7.3F Reference sensitivity for shared spectrum channel access 293

7.3F.1 General 293

7.3F.2 Reference sensitivity power level 293

7.3F.3 ΔRIB,c 294

7.3F.4 Intra-band contiguous shared spectrum channel access CA 295

7.3F.5 Inter-band CA with shared spectrum channel access 295

7.3F.5.1 Reference sensitivity exceptions due to UL harmonic interference 295

7.3F.5.2 Reference sensitivity exceptions due to receiver harmonic mixing 295

7.3F.5.3 Reference sensitivity exceptions due to cross band isolation 296

7.4 Maximum input level 296

7.4A Maximum input level for CA 297

7.4A.1 Maximum input level for Intra-band contiguous CA 297

7.4A.2 Maximum input level for Intra-band non-contiguous CA 297

7.4A.3 Maximum input level for Inter-band CA 297

7.4B Maximum input level for NR-DC 298

7.4D Maximum input level for UL MIMO 298

7.4E Maximum input level for V2X 298

7.4E.1 General 298

7.4E.2 Maximum input level for V2X con-current operation 298

7.5 Adjacent channel selectivity 298

7.5A Adjacent channel selectivity for CA 303

7.5A.1 Adjacent channel selectivity for Intra-band contiguous CA 303

7.5A.2 Adjacent channel selectivity Intra-band non-contiguous CA 305

7.5A.3 Adjacent channel selectivity Inter-band CA 306

7.5B Adjacent channel selectivity for NR-DC 306

7.5D Adjacent channel selectivity for UL MIMO 306

7.5E Adjacent channel selectivity for V2X 306

7.5E.1 General 306

7.5E.2 Adjacent channel selectivity for V2X con-current operation 307

7.5F Adjacent channel selectivity 307

7.5F.1 General 307

7.5F.2 Intra-band contiguous shared spectrum channel access CA 308

7.6 Blocking characteristics 309

7.6.1 General 309

7.6.2 In-band blocking 309

7.6.3 Out-of-band blocking 313

7.6.4 Narrow band blocking 316

7.6A Blocking characteristics for CA 317

7.6A.1 General 317

7.6A.2 In-band blocking for CA 317

7.6A.2.1 In-band blocking for Intra-band contiguous CA 317

7.6A.2.2 In-band blocking for Intra-band non-contiguous CA 318

7.6A.2.3 In-band blocking for Inter-band CA 318

7.6A.3 Out-of-band blocking for CA 319

7.6A.3.1 Out-of-band blocking for Intra-band contiguous CA 319

7.6A.3.2 Out-of-band blocking for Intra-band non-contiguous CA 320

7.6A.3.3 Out-of-band blocking for Inter-band CA 321

7.6A.4 Narrow band blocking for CA 322

7.6A.4.1 Narrow band blocking for Intra-band contiguous CA 322

7.6A.4.2 Narrow band blocking for Intra-band non-contiguous CA 322

7.6A.4.3 Narrow band blocking for Inter-band CA 323

7.6B Blocking characteristics for NR-DC 323

7.6C Blocking characteristics for SUL 323

7.6C.1 General 323

7.6C.2 In-band blocking for SUL 323

7.6C.3 Out-of-band blocking for SUL 323

7.6C.4 Narrow band blocking for SUL 324

7.6D Blocking characteristics for UL MIMO 324

7.6E Blocking characteristics for V2X 324

7.6E.1 General 324

7.6E.2 In-band blocking 324

7.6E.2.1 General 324

7.6E.2.2 In-band blocking for V2X con-current operation 325

7.6E.3 Out-of-band blocking 325

7.6E.3.1 General 325

7.6E.3.2 Out-of-band blocking for V2X con-current operation 326

7.6F Blocking characteristics 326

7.6F.1 General 326

7.6F.2 In-band blocking 326

7.6F.2.1 General 326

7.6F.2.2 Intra-band contiguous shared spectrum channel access CA 327

7.6F.3 Out-of-band blocking 328

7.6F.3.1 General 328

7.6F.3.2 Intra-band contiguous shared spectrum channel access CA 329

7.7 Spurious response 329

7.7A Spurious response for CA 331

7.7A.1 Spurious response for Intra-band contiguous CA 331

7.7A.2 Spurious response for Intra-band non-contiguous CA 331

7.7A.3 Spurious response for Inter-band CA 331

7.7B Spurious response for NR-DC 331

7.7D Spurious response for UL MIMO 332

7.7E Spurious response for V2X 332

7.7E.1 General 332

7.7E.2 Spurious response for V2X con-current operation 332

7.7F Spurious response for shared spectrum channel access 332

7.7F.1 General 332

7.7F.2 Intra-band contiguous shared spectrum channel access CA 333

7.8 Intermodulation characteristics 333

7.8.1 General 333

7.8.2 Wide band Intermodulation 333

7.8A Intermodulation characteristics for CA 336

7.8A.1 General 336

7.8A.2 Wide band intermodulation for CA 336

7.8A.2.1 Wide band intermodulation for Intra-band contiguous CA 336

7.8A.2.2 Wide band intermodulation for Intra-band non-contiguous CA 337

7.8A.2.3 Wide band intermodulation for Inter-band CA 337

7.8B Intermodulation characteristics for NR-DC 337

7.8D Intermodulation characteristics for UL MIMO 338

7.8E Intermodulation characteristics for V2X 338

7.8E.1 General 338

7.8E.2 Wide band Intermodulation 338

7.8E.2.1 General 338

7.8E.2.2 Wide band Intermodulation for V2X con-current operation 338

7.8F Intermodulation characteristics for shared spectrum channel access 338

7.8F.1 General 338

7.8F.2 Wide band Intermodulation 339

7.9 Spurious emissions 339

7.9A Spurious emissions for CA 340

7.9A.1 Void 340

7.9A.2 Void 340

7.9A.3 Spurious emissions for Inter-band CA 340

7.9B Spurious emissions for NR-DC 340

Annex A (normative): Measurement channels 341

A.1 General 341

A.2 UL reference measurement channels 341

A.2.1 General 341

A.2.2 Reference measurement channels 342

A.2.2.1 DFT-s-OFDM Pi/2-BPSK 342

A.2.2.2 DFT-s-OFDM QPSK 343

A.2.2.3 DFT-s-OFDM 16QAM 344

A.2.2.4 DFT-s-OFDM 64QAM 345

A.2.2.5 DFT-s-OFDM 256QAM 346

A.2.2.6 CP-OFDM QPSK 347

A.2.2.7 CP-OFDM 16QAM 349

A.2.2.8 CP-OFDM 64QAM 351

A.2.2.9 CP-OFDM 256QAM 353

A.2.3 Reference measurement channels for TDD 355

A.2.3.1 DFT-s-OFDM Pi/2-BPSK 355

A.2.3.2 DFT-s-OFDM QPSK 355

A.2.3.3 DFT-s-OFDM 16QAM 355

A.2.3.4 DFT-s-OFDM 64QAM 355

A.2.3.5 DFT-s-OFDM 256QAM 356

A.2.3.6 CP-OFDM QPSK 356

A.2.3.7 CP-OFDM 16QAM 356

A.2.3.8 CP-OFDM 64QAM 356

A.2.3.9 CP-OFDM 256QAM 357

A.3 DL reference measurement channels 358

A.3.1 General 358

A.3.2 DL reference measurement channels for FDD 359

A.3.2.1 General 359

A.3.2.2 FRC for receiver requirements for QPSK 359

A.3.2.3 FRC for maximum input level for 64QAM 361

A.3.2.4 FRC for maximum input level for 256 QAM 364

A.3.3 DL reference measurement channels for TDD 367

A.3.3.1 General 367

A.3.3.2 FRC for receiver requirements for QPSK 368

A.3.3.3 FRC for maximum input level for 64QAM 371

A.3.3.4 FRC for maximum input level for 256 QAM 374

A.4 CSI reference measurement channels 377

A.5 OFDMA Channel Noise Generator (OCNG) 377

A.5.1 OCNG Patterns for FDD 377

A.5.1.1 OCNG FDD pattern 1: Generic OCNG FDD Pattern for all unused REs 377

A.5.2 OCNG Patterns for TDD 377

A.5.2.1 OCNG TDD pattern 1: Generic OCNG TDD Pattern for all unused REs 377

A.6 Void 378

A.7 V2X reference measurement channels 378

A.7.1 General 378

A.7.2 FRC for V2X receiver requirements for QPSK 378

A.7.3 FRC for maximum input level for 64QAM 380

A.7.4 FRC for maximum input level for 256QAM 381

Annex B (informative): Void 383

Annex C (informative): Downlink physical channels 384

C.1 General 384

C.2 Setup 384

C.3 Connection 384

C.3.1 Measurement of Receiver Characteristics 384

Annex D (normative): Characteristics of the interfering signal 385

D.1 General 385

D.2 Interference signals 385

Annex E (normative): Environmental conditions 386

E.1 General 386

E.2 Environmental 386

E.2.1 Temperature 386

E.2.2 Voltage 387

E.2.3 Vibration 387

Annex F (normative): Transmit modulation 388

F.0 General 388

F.1 Measurement Point 388

F.2 Basic Error Vector Magnitude measurement 388

F.3 Basic in-band emissions measurement 389

F.4 Modified signal under test 389

F.5 Window length 392

F.5.1 Timing offset 392

F.5.2 Window length 392

F.5.3 Window length for normal CP 392

F.5.4 Window length for Extended CP 393

F.5.5 Window length for PRACH 394

F.6 Averaged EVM 395

F.7 Spectrum Flatness 396

Annex G (normative): 397

G.0 General 397

G.1 Measurement Point 397

G.2 Relative Phase Error Measurement 398

G.2.1 Symbols used 398

G.2.2 CFO (carrier frequency offset) correction 398

G.2.3 Steps of the measurement method 398

Annex H (informative): Void 399

Annex I (informative): Void 399

Annex J (informative): Void 399

Annex K (informative): Void 399

Annex L (normative): ModifiedMPR-Behavior 399

L.1 Indication of modified MPR behavior 399

Annex M (informative): Change history 401